**Knapsack Sprayer Operator Check List**

**Key** Checked/ Completed 3 Needs Attention x

Adjusted A Not Applicable na

Owner: Operator:

Make: Date:

**General Condition**

* Clean
* No apparent damage
* Strap fixing points secure

FILL WITH WATER

* Will straps take weight?
* Is sprayer stable when filled?

**Leakage Check**

* Check for leaks; upright and on side

**Function Check**

* Check pressure relief valve to max. limit
* Spray out – is cut-off valve working?
* Is spray pattern correct?
* Is nozzle undamaged?
* Is nozzle flow rate within 10% of manufacturer’s stated output?

**Internal Residue**

* Spray out until fan collapses and air appears
* Is remaining liquid less than cupful?

**Following Use**

* Rinse with detergent
* Rinse twice with water – flush out through lance
* Clean nozzle and all filters in water with soft brush
* Clean outside of tanks and straps
* Follow disposal procedure for rinsings

Comments/ Notes/ Specific items requiring attention

*Template provided by The Voluntary Initiative*